<?xml version="1.0"?>
<!DOCTYPE lmms-project>
<lmms-project creator="LMMS" creatorversion="1.3.0-alpha" type="instrumenttracksettings" version="28">
  <head/>
  <instrumenttracksettings muted="0" solo="0" type="0" mutedBeforeSolo="0" name="bonlag">
    <instrumenttrack vol="132.8" pitch="-797" enabled="0" scale="0" basenote="69" pitchrange="12" firstkey="0" enablecc="0" keymap="0" pan="-28" range_import="1" usemasterpitch="1" lastkey="127" mixch="6">
      <midicontrollers cc41="0" cc88="0" cc42="0" cc89="0" cc43="0" cc44="0" cc45="0" cc46="0" cc47="0" cc48="0" cc120="0" cc49="0" cc121="0" cc122="0" cc123="0" cc124="0" cc125="0" cc126="0" cc127="0" cc90="0" cc91="0" cc92="0" cc93="0" cc94="0" cc95="0" cc96="0" cc50="0" cc97="0" cc51="0" cc98="0" cc52="0" cc99="0" cc53="0" cc54="0" cc55="0" cc56="0" cc57="0" cc10="0" cc58="0" cc11="0" cc59="0" cc12="0" cc13="0" cc14="0" cc15="0" cc16="0" cc17="0" cc18="0" cc19="0" cc0="0" cc1="0" cc2="0" cc3="0" cc4="0" cc5="0" cc6="0" cc7="0" cc8="0" cc60="0" cc9="0" cc61="0" cc62="0" cc63="0" cc64="0" cc65="0" cc66="0" cc20="0" cc67="0" cc21="0" cc68="0" cc22="0" cc69="0" cc23="0" cc24="0" cc25="0" cc26="0" cc27="0" cc28="0" cc100="0" cc29="0" cc101="0" cc102="0" cc103="0" cc104="0" cc105="0" cc106="0" cc107="0" cc108="0" cc109="0" cc70="0" cc71="0" cc72="0" cc73="0" cc74="0" cc75="0" cc76="0" cc30="0" cc77="0" cc31="0" cc78="0" cc32="0" cc79="0" cc33="0" cc34="0" cc35="0" cc36="0" cc37="0" cc38="0" cc110="0" cc39="0" cc111="0" cc112="0" cc113="0" cc114="0" cc115="0" cc116="0" cc117="0" cc118="0" cc119="0" cc80="0" cc81="0" cc82="0" cc83="0" cc84="0" cc85="0" cc86="0" cc40="0" cc87="0"/>
      <instrument name="nes">
        <nes envloop1="0" sweep1="0" vibr="0" envloop2="0" sweep2="0" nmode4="0" envloop4="0" crs1="0" crs2="0" crs3="0" nswp4="0" on1="0" on2="0" on3="1" dc1="0" on4="0" dc2="2" nfreq4="0" swrate1="0" vol1="15" vol2="15" swamt1="0" swrate2="0" swamt2="0" vol3="15" vol="1" vol4="2" envlen1="0" envlen2="0" nfrqmode4="0" envlen4="0" envon1="0" envon2="0" nq4="1" envon4="0">
          <key/>
        </nes>
      </instrument>
      <eldata ftype="12" fcut="336" fwet="1" fres="7.3399997">
        <elvol userwavefile="" ctlenvamt="0" lspd_syncmode="0" lshp="0" x100="0" rel="0.1" dec="0.5" sustain="0.5" lspd="0.1" lpdel="0" att="0" pdel="0" lspd_denominator="4" hold="0.22400001" amt="0" latt="0" lspd_numerator="4" lamt="0"/>
        <elcut userwavefile="" ctlenvamt="0" lspd_syncmode="0" lshp="0" x100="0" rel="0.1" dec="0.5" sustain="0.5" lspd="0.1" lpdel="0" att="0" pdel="0" lspd_denominator="4" hold="0.5" amt="0" latt="0" lspd_numerator="4" lamt="0"/>
        <elres userwavefile="" ctlenvamt="0" lspd_syncmode="0" lshp="0" x100="0" rel="0.1" dec="0.5" sustain="0.5" lspd="0.1" lpdel="0" att="0" pdel="0" lspd_denominator="4" hold="0.5" amt="0" latt="0" lspd_numerator="4" lamt="0"/>
      </eldata>
      <chordcreator chord="0" chord-enabled="0" chordrange="2"/>
      <arpeggiator arpcycle="0" arpmiss="0" arpmode="0" arptime_numerator="4" arpskip="0" arptime="200" arprange="2" arpgate="100" arprepeats="1" arpdir="0" arp="0" arptime_denominator="4" arp-enabled="0" arptime_syncmode="0"/>
      <midiport readable="0" basevelocity="63" writable="0" inputcontroller="-1" outputcontroller="-1" fixedinputvelocity="-1" inputchannel="0" outputchannel="1" fixedoutputvelocity="-1" outputprogram="1" fixedoutputnote="-1"/>
      <fxchain enabled="1" numofeffects="2">
        <effect autoquit_syncmode="0" on="0" autoquit_denominator="4" autoquit="1" autoquit_numerator="4" wet="1" gate="0" name="ladspaeffect">
          <ladspacontrols ports="4">
            <port02 data="0.0049999999"/>
            <port03 data="0.37450001"/>
            <port04 data="0.00050000002"/>
            <port05 data="0.25"/>
          </ladspacontrols>
          <key>
            <attribute value="caps" name="file"/>
            <attribute value="Plate2x2" name="plugin"/>
          </key>
        </effect>
        <effect autoquit_syncmode="0" on="1" autoquit_denominator="4" autoquit="1" autoquit_numerator="4" wet="1" gate="0" name="ladspaeffect">
          <ladspacontrols ports="5">
            <port04 data_syncmode="0" data="10" data_denominator="4" data_numerator="4"/>
            <port05 data="0.384"/>
            <port06 data_syncmode="0" data="10" data_denominator="4" data_numerator="4"/>
            <port07 data="0.35999998"/>
            <port08 data="1"/>
          </ladspacontrols>
          <key>
            <attribute value="cmt" name="file"/>
            <attribute value="canyon_delay" name="plugin"/>
          </key>
        </effect>
      </fxchain>
    </instrumenttrack>
  </instrumenttracksettings>
</lmms-project>
