<?xml version="1.0"?>
<!DOCTYPE lmms-project>
<lmms-project creator="LMMS" creatorversion="1.3.0-alpha" type="instrumenttracksettings" version="28">
  <head/>
  <instrumenttracksettings name="Xpressive" solo="0" muted="0" mutedBeforeSolo="0" type="0">
    <instrumenttrack basenote="69" enabled="1" enablecc="0" vol="40.799999" firstkey="0" mixch="3" pitch="-82" scale="0" usemasterpitch="1" pitchrange="1" pan="0" keymap="0" lastkey="127" range_import="1">
      <midicontrollers cc60="0" cc61="0" cc62="0" cc63="0" cc64="0" cc65="0" cc66="0" cc20="0" cc67="0" cc21="0" cc68="0" cc22="0" cc69="0" cc120="0" cc23="0" cc121="0" cc24="0" cc122="0" cc25="0" cc123="0" cc26="0" cc124="0" cc27="0" cc125="0" cc28="0" cc126="0" cc29="0" cc127="0" cc70="0" cc71="0" cc72="0" cc73="0" cc74="0" cc75="0" cc76="0" cc30="0" cc77="0" cc31="0" cc78="0" cc32="0" cc79="0" cc33="0" cc34="0" cc35="0" cc36="0" cc37="0" cc38="0" cc39="0" cc0="0" cc1="0" cc2="0" cc80="0" cc3="0" cc81="0" cc4="0" cc82="0" cc5="0" cc83="0" cc6="0" cc84="0" cc7="0" cc85="0" cc8="0" cc86="0" cc9="0" cc40="0" cc87="0" cc41="0" cc88="0" cc42="0" cc89="0" cc43="0" cc44="0" cc45="0" cc46="0" cc47="0" cc48="0" cc49="0" cc100="0" cc101="0" cc102="0" cc103="0" cc104="0" cc105="0" cc106="0" cc107="0" cc108="0" cc109="0" cc90="0" cc91="0" cc92="0" cc93="0" cc94="0" cc95="0" cc96="0" cc50="0" cc97="0" cc51="0" cc98="0" cc52="0" cc99="0" cc53="0" cc54="0" cc55="0" cc56="0" cc57="0" cc10="0" cc58="0" cc11="0" cc59="0" cc12="0" cc110="0" cc13="0" cc111="0" cc14="0" cc112="0" cc15="0" cc113="0" cc16="0" cc114="0" cc17="0" cc115="0" cc18="0" cc116="0" cc19="0" cc117="0" cc118="0" cc119="0"/>
      <instrument name="xpressive">
        <xpressive W2="" W3="" W3sample="[encoded data, 21848 characters]" W2sample="[encoded data, 21848 characters]" W1sample="[encoded data, 21848 characters]" interpolateW1="0" smoothW1="0" interpolateW2="0" interpolateW3="0" O1="expw(integrate(f*2))&#xa;&#xa;&#xa;squarew(integrate(f*A1+last(100*A3)))&#xa;&#xa;&#xa;" smoothW2="0" O2="" smoothW3="0" version="0.1" RELTRANS="50" A1="-0.65999997" A2="-0.049999997" A3="-0.17999999" PAN1="0" PAN2="0" W1="">
          <key/>
        </xpressive>
      </instrument>
      <eldata fcut="1177" ftype="8" fwet="1" fres="1.3399999">
        <elvol ctlenvamt="0" latt="0" lamt="0.31999999" lspd_numerator="4" lspd_syncmode="0" sustain="0.5" lshp="0" lpdel="0" x100="0" rel="0.1" lspd_denominator="4" dec="0.5" userwavefile="" lspd="0.1" att="0" pdel="0" hold="0.5" amt="0"/>
        <elcut ctlenvamt="0" latt="0" lamt="0.47999999" lspd_numerator="4" lspd_syncmode="0" sustain="0.5" lshp="0" lpdel="0" x100="0" rel="0.1" lspd_denominator="4" dec="0.5" userwavefile="" lspd="0.1" att="0" pdel="0" hold="0.5" amt="0"/>
        <elres ctlenvamt="0" latt="0" lamt="0" lspd_numerator="4" lspd_syncmode="0" sustain="0.5" lshp="0" lpdel="0" x100="0" rel="0.1" lspd_denominator="4" dec="0.5" userwavefile="" lspd="0.1" att="0" pdel="0" hold="0.5" amt="0"/>
      </eldata>
      <chordcreator chord-enabled="0" chord="0" chordrange="1"/>
      <arpeggiator arptime_denominator="4" arp-enabled="0" arprange="1" arptime_syncmode="0" arptime_numerator="4" arpmiss="0" arpmode="0" arpskip="0" arptime="200" arpgate="100" arp="0" arprepeats="1" arpcycle="0" arpdir="0"/>
      <midiport inputchannel="0" fixedoutputvelocity="-1" outputcontroller="-1" fixedinputvelocity="-1" outputchannel="1" fixedoutputnote="-1" outputprogram="1" basevelocity="63" readable="0" inputcontroller="-1" writable="0"/>
      <fxchain numofeffects="3" enabled="1">
        <effect autoquit_syncmode="0" name="amplifier" autoquit="1" on="0" autoquit_numerator="4" autoquit_denominator="4" wet="1" gate="0">
          <AmplifierControls volume="200" left="100" pan="0" right="100"/>
          <key/>
        </effect>
        <effect autoquit_syncmode="0" name="amplifier" autoquit="1" on="0" autoquit_numerator="4" autoquit_denominator="4" wet="1" gate="0">
          <AmplifierControls volume="200" left="100" pan="0" right="100"/>
          <key/>
        </effect>
        <effect autoquit_syncmode="0" name="ladspaeffect" autoquit="1" on="0" autoquit_numerator="4" autoquit_denominator="4" wet="1" gate="0">
          <ladspacontrols ports="4">
            <port00 data="18.84"/>
            <port01 data="8.5200005"/>
            <port02 data="0"/>
            <port03 data="0.0079999994"/>
          </ladspacontrols>
          <key>
            <attribute name="file" value="tap_rotspeak"/>
            <attribute name="plugin" value="tap_rotspeak"/>
          </key>
        </effect>
      </fxchain>
    </instrumenttrack>
  </instrumenttracksettings>
</lmms-project>
