<?xml version="1.0"?>
<!DOCTYPE lmms-project>
<lmms-project creatorversion="1.3.0-alpha" version="28" creator="LMMS" type="instrumenttracksettings">
  <head/>
  <instrumenttracksettings muted="0" name="Xpressive" mutedBeforeSolo="0" solo="0" type="0">
    <instrumenttrack pitch="-352" scale="0" keymap="0" pan="0" basenote="69" usemasterpitch="1" enablecc="0" firstkey="0" lastkey="127" enabled="1" mixch="0" range_import="1" pitchrange="6" vol="98.400002">
      <midicontrollers cc70="0" cc71="0" cc72="0" cc73="0" cc74="0" cc75="0" cc76="0" cc30="0" cc77="0" cc31="0" cc78="0" cc32="0" cc79="0" cc33="0" cc34="0" cc35="0" cc36="0" cc37="0" cc38="0" cc39="0" cc100="0" cc101="0" cc80="0" cc102="0" cc81="0" cc103="0" cc82="0" cc104="0" cc83="0" cc105="0" cc84="0" cc106="0" cc85="0" cc107="0" cc86="0" cc108="0" cc40="0" cc87="0" cc109="0" cc41="0" cc88="0" cc42="0" cc89="0" cc43="0" cc44="0" cc45="0" cc46="0" cc47="0" cc48="0" cc49="0" cc110="0" cc111="0" cc90="0" cc112="0" cc91="0" cc113="0" cc92="0" cc114="0" cc93="0" cc115="0" cc94="0" cc116="0" cc95="0" cc117="0" cc96="0" cc118="0" cc50="0" cc97="0" cc119="0" cc51="0" cc98="0" cc52="0" cc99="0" cc53="0" cc54="0" cc55="0" cc56="0" cc57="0" cc10="0" cc58="0" cc11="0" cc59="0" cc0="0" cc12="0" cc1="0" cc13="0" cc2="0" cc14="0" cc3="0" cc15="0" cc4="0" cc16="0" cc5="0" cc17="0" cc6="0" cc18="0" cc7="0" cc19="0" cc8="0" cc9="0" cc120="0" cc121="0" cc122="0" cc123="0" cc124="0" cc125="0" cc126="0" cc127="0" cc60="0" cc61="0" cc62="0" cc63="0" cc64="0" cc65="0" cc66="0" cc20="0" cc67="0" cc21="0" cc68="0" cc22="0" cc69="0" cc23="0" cc24="0" cc25="0" cc26="0" cc27="0" cc28="0" cc29="0"/>
      <instrument name="xpressive">
        <xpressive O1="expw( integrate(f+A2) + sinew( integrate(f+A1) ) )" O2="" W3sample="[encoded data, 21848 characters]" interpolateW1="0" W2sample="[encoded data, 21848 characters]" A1="-0.98999995" interpolateW2="0" PAN1="0" W1sample="[encoded data, 21848 characters]" A2="0.71999997" interpolateW3="0" PAN2="0" A3="0.059999999" version="0.1" smoothW1="0" smoothW2="0" smoothW3="0" RELTRANS="50" W1="trianglew(t)" W2="randv(t * srate)" W3="">
          <key/>
        </xpressive>
      </instrument>
      <eldata ftype="0" fres="0.41" fcut="2240" fwet="1">
        <elvol lshp="0" rel="0.39600003" x100="0" lpdel="0" dec="0.58400005" sustain="0.24800001" att="0.056000002" lspd_syncmode="0" lspd="0.1" pdel="0" amt="1" hold="0.14" userwavefile="" ctlenvamt="0" lspd_numerator="4" latt="0" lamt="0" lspd_denominator="4"/>
        <elcut lshp="0" rel="0.1" x100="0" lpdel="0" dec="0.5" sustain="0.5" att="0" lspd_syncmode="0" lspd="0.21599999" pdel="0" amt="0" hold="0.084000006" userwavefile="" ctlenvamt="0" lspd_numerator="4" latt="0" lamt="0.71999997" lspd_denominator="4"/>
        <elres lshp="0" rel="0.1" x100="0" lpdel="0" dec="0.5" sustain="0.5" att="0" lspd_syncmode="0" lspd="0.1" pdel="0" amt="0" hold="0.5" userwavefile="" ctlenvamt="0" lspd_numerator="4" latt="0" lamt="0" lspd_denominator="4"/>
      </eldata>
      <chordcreator chord="0" chordrange="1" chord-enabled="0"/>
      <arpeggiator arpskip="0" arptime_denominator="4" arptime="200" arprepeats="1" arpcycle="0" arpgate="100" arp-enabled="0" arptime_numerator="4" arptime_syncmode="0" arpdir="0" arprange="1" arp="0" arpmiss="0" arpmode="0"/>
      <midiport inputchannel="0" fixedoutputvelocity="-1" readable="0" writable="0" fixedoutputnote="-1" outputchannel="1" outputcontroller="-1" outputprogram="1" basevelocity="63" inputcontroller="-1" fixedinputvelocity="-1"/>
      <fxchain enabled="1" numofeffects="3">
        <effect autoquit_syncmode="0" autoquit_numerator="4" gate="0" name="ladspaeffect" autoquit="1" wet="1" autoquit_denominator="4" on="1">
          <ladspacontrols ports="12" link="1">
            <port01 data_numerator="4" link="1" data_syncmode="0" data_denominator="4">
              <data scale_type="log" id="6857186" value="5"/>
            </port01>
            <port02 data_numerator="4" data="3.9781249" link="1" data_syncmode="0" data_denominator="4"/>
            <port03 data="2.6299999" link="1"/>
            <port04 data="1" link="1"/>
            <port05 data="0.25" link="1"/>
            <port06 data="0" link="1"/>
            <port11 data_numerator="4" data_syncmode="0" data_denominator="4">
              <data scale_type="log" id="570246" value="5"/>
            </port11>
            <port12 data_numerator="4" data="3.9781249" data_syncmode="0" data_denominator="4"/>
            <port13 data="2.6299999"/>
            <port14 data="1"/>
            <port15 data="0.25"/>
            <port16 data="0"/>
          </ladspacontrols>
          <key>
            <attribute name="file" value="caps"/>
            <attribute name="plugin" value="ChorusI"/>
          </key>
        </effect>
        <effect autoquit_syncmode="0" autoquit_numerator="4" gate="0" name="ladspaeffect" autoquit="1" wet="1" autoquit_denominator="4" on="0">
          <ladspacontrols ports="12">
            <port07>
              <data scale_type="log" id="313748" value="0.98984641"/>
            </port07>
            <port08>
              <data scale_type="log" id="426408" value="6324.5552"/>
            </port08>
            <port09 data="2"/>
            <port010 data="1"/>
            <port011 data="0.5"/>
            <port012 data="1"/>
            <port013 data="0"/>
            <port014>
              <data scale_type="log" id="2985196" value="632.45551"/>
            </port014>
            <port015>
              <data scale_type="log" id="1987121" value="3556.5579"/>
            </port015>
            <port016 data="1"/>
            <port017 data="1"/>
            <port018 data="1"/>
          </ladspacontrols>
          <key>
            <attribute name="file" value="veal"/>
            <attribute name="plugin" value="Reverb"/>
          </key>
        </effect>
        <effect autoquit_syncmode="0" autoquit_numerator="4" gate="0" name="ladspaeffect" autoquit="1" autoquit_denominator="4" wet="1" on="1">
          <ladspacontrols ports="16" link="1">
            <port00 data="12600.37" link="1"/>
            <port01 data="0.79999995" link="1"/>
            <port02 data="10000.5" link="1"/>
            <port03 data="0" link="1"/>
            <port04 data="15000.25" link="1"/>
            <port05 data="0" link="1"/>
            <port06 data="20000" link="1"/>
            <port07 data="0" link="1"/>
            <port10 data="12600.37"/>
            <port11 data="0.79999995"/>
            <port12 data="10000.5"/>
            <port13 data="0"/>
            <port14 data="15000.25"/>
            <port15 data="0"/>
            <port16 data="20000"/>
            <port17 data="0"/>
          </ladspacontrols>
          <key>
            <attribute name="file" value="phasers_1217"/>
            <attribute name="plugin" value="fourByFourPole"/>
          </key>
        </effect>
      </fxchain>
    </instrumenttrack>
  </instrumenttracksettings>
</lmms-project>
